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Introduction:
The Construction Traffic / Site Traffic Management Plan specifies the requirement and objectives concerning the method of site operation which shall be observed at all times during the fulfilment of the site. The site can be accessed from the East, which is located to the right hand side of Derby Road, when approaching from the A50. There are nearby agricultural fields to the North, surrounding this new development and adjacent to the site, are existing residential developments.

The site is located on Derby Road, to the eastern side of Hilton village. The land is currently used for agricultural purposes and is not subject to any notable planning history.
The application site comprises 2.68 hectares of land.
The site WILL ONLY be accessed via Derby Road. 

Sequence of Works:
Preliminary site preparation works required to be carried out on mobilisation on site shall be completed as soon as possible. In particular, the Site Manager shall:-

· Establish site accommodation- site office, amenity facilities and services; site compound.

· Establish a temporary Show Home with mains electricity, water and drainage.

· Erect specified boundary, screening and protective fencing upon commencement on site.

· Ensure that all site personnel are instructed regarding access and specified restrictions.

Site Personnel Car Parking:
Staff and contractor parking will be located within the site boundary, adjacent to the Site Compound. It is the responsibility of the Site Manager to ensure that all site personnel utilise the car parking facilities, and that at no time should site personnel park on the public highway. The provision of on-site parking will remove the risk of contractor parking on the local highway network.

Security Fencing:
Security fencing will be provided to all build areas and will be adjusted as the build progresses.

Sequence Guidelines:
Plot super-structure works shall not be commenced until main road works, including drains, kerbing and base tarmac shall be complete to accommodate correct unloading and storage. And the foul and surface water drainage, including manholes and main drainage connections; gulley to drive; foundations and brickwork.

Maintenance:
The Site Manager and Sales Adviser shall monitor the condition of each show home and ‘signed off units’ on a weekly basis. When wear and tear requires remedial works to be carried out, the Site Manager and/or Sales Advisor shall make appropriate arrangements for this to be done.

Site Cleanliness:
The Site Manager will at all times maintain a high standard of presentation and general tidiness throughout the site.

Noise/Vibration:

During construction, the principles of the “best practicable means” (BPM), as defined in the Control of Pollution Act 1974 would be used to minimise emissions throughout the construction period. This would incorporate the use of measures to control noise and vibration, and the use of working methods that result in minimum effects compatible with normal working practices. To control noise emissions from construction activities, standard measures by Bellway Homes Ltd., would normally include:

· Any works for the erection, construction, alteration, repair or maintenance of buildings, structures or roads; or the breaking up, opening or boring under any road or adjacent land in connection with the construction, inspection, maintenance or removal of works in connection with this development, shall only take place during permitted hours.

· Goods vehicles shall only be permitted to make deliveries of materials and equipment to the site or to remove materials and equipment from the site during the permitted site operating hours. 

· No site generators, pumps or other site equipment will be operated outside of the permitted operating hours ( unless, their use has been agreed in advance by the local authority and agreed mitigation measures are in  place ).

· The guidance given in BS5228:2014, Parts 1 and 2, “Code of practice for noise and vibration control on construction and open sites”, will be taken into account when assessing the impacts of construction noise.

· Selection of inherently quiet plant;

· The use, where necessary and practicable, of hoardings, screens or barriers to be sited between noisy construction activities/plant;

· Avoid unnecessary revving of engines and switch off equipment when not required. 

· Use rubber linings in, for example, chutes and dumpers to reduce impact noise. 

· Minimise the drop height of materials where possible;

· Start plant and vehicles sequentially rather than all together; 

· No works to take place during hours outside of those agreed with the LPA;

· Noisy activities and plant to be reviewed and substituted where possible;

· Portable acoustic hoardings and barriers and enclosures for significantly noisy plant, for example compressors, to be used where possible. 
· Regular maintenance and the use of equipment to be in accordance with manufacturer’s instructions;

· Plant to be switched off whilst not in use;

· Deliveries to arrive during normal site hours and engines to be switched off whilst unloading.
The above range of noise controls represents the measures that are regularly and successfully applied to large scale construction projects in order to minimise noise effects on local communities.

General control measures for road cleaning and dust suppression:
Monitor weather reports to ensure appropriate dust suppression and road cleaning is available when required.

Mud on roads:
· Sweepers to be employed to clean site and adjacent roads

· Labourer to clean large debris immediately

· Only designated routes are to be used- site directions to be provided to suppliers and sub-contractor vehicles. Please see Construction Route Plan.

· Road sweepers will be used to keep the main development road clean and to maintain clean access from the adjoining roads. A temporary wheel washing facility will be in operation when and where necessary until the site reaches the stage where this is no longer required.
· A Jet Wash wheel washing facility will be in operation when and where necessary 
Dust and Emissions:
Specific issues to vehicles entering and leaving the site will include:

· Easily cleaned hard standing areas for vehicles

· Maintain haul roads and hard standing by regular brushing and water spraying

· All vehicles carrying soil and other dusty materials to be fully sheeted

· Enforce site speed limits

Other Construction Dust & Suppression measures:
Generally, Construction Dust comes in the form of;

Silica Dust – this type of dust is created when working on silica containing materials like concrete, mortar and sandstone. 

Wood Dust – created when working with softwood, hardwood and wood-based products like MDF and plywood.

Lower Toxicity Dusts – generally created when working with materials containing very little or no silica, with the most common being gypsum ( eg. In plasterboard ), limestone, marble and dolomite.
When general on-site construction works are taking place, Bellway Homes Ltd. endeavours to assess the risks of dust, i.e, the type of tasks in hand, work environments, time taken to carry out the various tasks, frequency etc., and then put in place, measures ( as necessary ), to ensure dust levels are kept to a minimum. 
This is carried out by either, the use of water ( damping down dust clouds when using certain tools / equipment ) or the on-tool extraction method ( removes dust as it is being produced. The extraction method, is a type of exhaust ventilation ( LEV ) system that fits directly to the tool. The extraction unit is used for High, Medium and Low class filter units accordingly.

In addition, where Water or on-tool extraction not always appropriate, Respiratory Protective Equipment (RPE) is used by staff, as a further protective measure.
Other dust control measures in place, include enclosing the work area to stop dust escaping by use of sheething and temporary screens, general mechanical ventilation to remove dusty air from the work area and the use of appropriate work clothing that do not keep hold of the dust. 
Furthermore, through regular training of Bellway’s staff, we ensure that workers are carrying out the works in the right way and using tools/equipment, correctly. Training would include, dust risks in general and its effects on health, how to use dust controls and check that they are working, maintained and equipment kept clean, how to use and look after RPE and other Personal Protective Equipment (PPE). In addition to staff training, regular checks are made to ensure controls are in full working condition, so that controls are effective. 

Through regular training and supervision, general dust on site, is kept to a minimum.
Units under construction:
The Site Manager will ensure that each and every trade leaves units under construction clean and tidy at the end of each working day and should include the restacking and protection of materials.
Rubbish Skips:
All sites will be operating a waste segregation policy, which is to be adhered to. Rubbish skips shall be provided sufficient to maintain the site in a neat and tidy state.

Unloading and Storage of Construction Materials:
The Site Manager shall be responsible for the unloading, checking, protecting and handling of all materials delivered to site. It is also the Site Managers responsibility to ensure that materials supplied by Bellway Homes are thoroughly checked on arrival on site and that the necessary recording and reporting in respect of quality and quantity against the inventory are carried out.
Bricks, blocks, tiles and lintels shall be offloaded and stacked in neat piles above ground level on pallets on level ground and covered. They shall be positioned off the main roads and footpaths and either adjacent to the appropriate plots or in the front gardens, or alternatively stored within the site compound.
Waste Management:
Bellway Homes operates a waste management policy. The policy will be achieved by:

· Assigning responsibility for waste management to the appropriate Site Manager.
· Minimising the use of material resources and the production of waste through, by way of efficient design, logistics, stock control, the use of prefabricated/pre-sized materials, minimising packaging and efficient construction techniques.
· Ensuring that our sub contractors and waste management contractors manage waste properly and maximise recycling.
· Develop and implement Waste Management Plans for our sites in line with good practise.
· Whenever possible, maximising the re-use, recycling and recovery of construction, demolition and excavation waste on site.
· We encourage the segregation of waste on site where practical, in order to recycle waste and reduce waste disposal costs.

In addition, the company carries out a regional and national waste/recycling report to continually monitor the standards being achieved.
Routing of Construction Vehicles/Deliveries:
The routing of Construction vehicles and deliveries, are to be made via Derby Road off either the A50 or A38. 

Restrictions

Site Manager to ensure no burning of materials to be carried out on site during the construction phase of the development, including any preparatory works to clear vegetation on site.

No generators shall be used on the site during the construction phase until details have been submitted to and approved in writing by the Local Planning Authority.  Thereafter, only those approved generators shall be used.

Delivery & Working Hours:
Delivery Hours and Working Hours, including demolition and construction works will be restricted to between:

Mondays to Fridays 0800 hours to 1800 hours;

Saturday 0800 hours to 1300 hours;

No working on Sundays or Public Holidays, except for works to address an emergency.
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