Design & Access Statement
38 Regent Street

CHURCH GRESLEY – Swadlincote DE11 9PL

Context analysis

The existing premises comprise a detached dwelling house on a residential street with small forecourt area and extensive rear garden.

The house is of traditional brick construction, with slate roof.  The main part of the house is two storeys in height, with converted loft.

At the rear of the premises the kitchen and outbuildings form one continuous single storey structure. 

A passageway to the west side gives access to the rear yard and garden. Access to the front is generally level, with only standard front entrance doorstep.

Amount

The floor space usage currently is residential. The floor space to the rear, single storey area, will be increased in size.  The main house will remain unchanged.

Layout

The layout of the main house will remain unchanged.  A new layout is proposed for the rear, extended kitchen and utility area.

Scale

The proposed extension will enlarge the size of the kitchen, being wider than the current single storey structure.  the side walls will not extend beyond the main house walls.  The proposed roof will be higher than the current single storey roof – and will be monopitch in style.  It is considered that the extension will be suitably in proportion with the current house and will not appear to be excessive in size.
Appearance

The new extension will be built using materials which will match the current house.  Bricks and slates will be chosen to match the existing walls and roof as closely as possible.  New windows will match existing windows.

The proposed monopitch roof will be positioned to suit the position of the existing rear window.

Landscaping

There are no landscaping works included in the proposed development
Proposed works and objectives
The proposal comprises the construction of a rear extension – to replace the existing, smaller single storey kitchen and utility accommodation. 

The existing east side wall, which is located on the property boundary, will be retained and extended.  New windows and doors are proposed to the south and west sides of the new building, in line with the current design. 

The new extension is intended to provide improved kitchen and utility space.  

Design

The new building will be constructed using bricks and slates to match the existing house as closely as possible.  New windows, gutters and downpipes will also match existing fixtures in colour and material.  The proposed development will not alter the front elevation of the house in any way.  
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